**Safe warning**


1, Check supply voltage whether it matches the light engine

2,Prohibit to place the light engine under rain or wet spot, prevent from causing troubles or danger


of electronic shock


3,Light engine should be used in droughty surroundings, not stack other things around it


|  |  |  |  |
| --- | --- | --- | --- |
| Iutput voltage | 12VDC | Power frequency | NONE |
| Quantity of LED | 1pcs | Color Control | 2.4G remote control |
| Color | RGBW | twinke wheel control | RF remote control |
| Life of LED | 50000H | Body size | L150\*W150\*H88MM (without connector) |
| RED | 180LM | Gear | inside |
| Green | 360LM | LED brand | EPILEDS |
| Blue | 90LM | Connector diameter: | 30mm |
| White | 390LM | Operate temperature | -10-40°C |
| Max power | 27W | Body size | L150\*W150\*H88MM (without connector) |




**Color control(2.4G remote control)**












**Color program list**



**Twinkle wheel control(RF remote control)**

****